Format for This Application,Data for 2D. No specific Instrument. Extension is not specified,1) **.rm2 **.rmo2 **.rmo  (Required)
Bruker FID Data,Following files should be in one folder. Only one data in a folder.,1) ser  (Data File:Required),2) acqus  (Required),3) acqu2s  (Required),4) acqu,5) acqu2,6) Spec.BRUF  (note 2)
Bruker Spectrum Data,Following files should be in one folder. Only one data in a folder.,1) 2rr  (Data File:Required),2) 2ri,3) 2ir,4) 2ii,5) procs  (Required),6) proc2s  (Required),7) proc,8) proc2,9) parm.text,10) title,11) Spec.BRUD   (note 2)
JEOL Alice2/Excalibur/AL,,1) ***.als  (Required)
JEOL GX/GSX/EX,Spectrum Data or FID data for absolute measurement. Following filesshould be paired. "***" is the same name.,1) ***.GXD  (Data file:Required),2) ***.GXP  (Required)
JEOL GX/GSX/EX(PhaseSensitive),FID data for phase sensituve measurement. Following filesshould be paired. "***" is the same name.,1) ***01.GXD  (Data File:Required),2) ***02.GXD  (Data File:Required),3) ***01.GXP  (Required),4) ***02.GXP  (Required)
JEOL AlphaSpectrum data,In some case a number may follow the extension,1) ***.nmd  (Required)
JEOL Alpha FID Data,In some case a number may follow the extension,1) ***.nmf  (Required)
JEOL LambdaSpectrum Data,,1) ***.nmdata  (Required)
JEOL Lambda FID Data,,1) ***.nmfid  (Required)
JEOL Delta/ECP/ECA,No Specific extension,1) ***.*  (Required)
Varian Unity/Unix FID Data,Following files should be in one folder. Only one data in a folder.,1) fid  (Data File:Required),2) procpar  (Required),3) text,4) Spec.VarF  (note 2)
Varian Unity/Unix Spectrum Data,Following files should be in one folder. Only one data in a folder.,1) data  (Data File:Required),2) curpar (Required),3) procpar,4) text,5) Spec.VarD  (note 2)
